From d43547a64111da6fb4cba322c8675176bddf8622 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Fri, 7 Aug 2015 23:59:33 -0500
Subject: [PATCH 103/143] northbridge/amd/amdmct/mct_ddr3: Force retraining on
 every boot

Change-Id: I017e0dd5120110124d5b5d5276befef6f7740614
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/northbridge/amd/amdmct/mct_ddr3/mct_d.c |   10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
index 2ca65ca..330f37f 100644
--- a/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
+++ b/src/northbridge/amd/amdmct/mct_ddr3/mct_d.c
@@ -1735,6 +1735,16 @@ restartinit:
 					allow_config_restore = 0;
 		}
 
+		/* FIXME
+		 * Stability issues have arisen on multiple Family 15h systems
+		 * when configuration restoration is enabled.  In all cases these
+		 * stability issues resolved by allowing the RAM to go through a
+		 * full training cycle.
+		 *
+		 * Debug and reenable this!
+		 */
+		allow_config_restore = 0;
+
 		for (Node = 0; Node < MAX_NODES_SUPPORTED; Node++) {
 			struct DCTStatStruc *pDCTstat;
 			pDCTstat = pDCTstatA + Node;
-- 
1.7.9.5

