From 60a55771f802ef5c3fa3b080e7d130ca24acab45 Mon Sep 17 00:00:00 2001
From: Timothy Pearson <tpearson@raptorengineeringinc.com>
Date: Thu, 4 Jun 2015 00:07:05 -0500
Subject: [PATCH 042/143] cpu/amd/car: Initialize entire CAR space instead of
 only half

Change-Id: If2b6c875e523f595e662d5d62322c3c3f96ccb4a
Signed-off-by: Timothy Pearson <tpearson@raptorengineeringinc.com>
---
 src/cpu/amd/car/cache_as_ram.inc |    4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/src/cpu/amd/car/cache_as_ram.inc b/src/cpu/amd/car/cache_as_ram.inc
index 4ccde3f..9edc41f 100644
--- a/src/cpu/amd/car/cache_as_ram.inc
+++ b/src/cpu/amd/car/cache_as_ram.inc
@@ -460,12 +460,12 @@ fam10_end_part1:
 	/* Read the range with lodsl. */
 	cld
 	movl	$CacheBase, %esi
-	movl	$(CacheSize >> 2), %ecx
+	movl	$CacheSize, %ecx
 	rep	lodsl
 
 	/* Clear the range. */
 	movl	$CacheBase, %edi
-	movl	$(CacheSize >> 2), %ecx
+	movl	$CacheSize, %ecx
 	xorl	%eax, %eax
 	rep	stosl
 
-- 
1.7.9.5

