(export (version D)
  (design
    (source /home/user/QubesIncoming/crypto/pcb/hisolator/vl670/vl670/vl670.sch)
    (date "Thu Sep 23 01:47:17 2021")
    (tool "Eeschema 5.1.10-6.fc33")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Main Schematic - VL670 Development Board")
        (company "Copyright (C) 2021 Tom Li (niconiconi)")
        (rev v0.01-dev)
        (date 2021-06-29)
        (source vl670.sch)
        (comment (number 1) (value https://creativecommons.org/publicdomain/zero/1.0/))
        (comment (number 2) (value "the designer has waived all copyright and related or neighboring rights."))
        (comment (number 3) (value "To the extent possible under law,"))
        (comment (number 4) (value "License: CC 0, “No Rights Reserved”"))))
    (sheet (number 2) (name "/USB AC CAP/ESD/MUX/") (tstamps /60085564/)
      (title_block
        (title "USB-C Schematic - VL670 Development Board")
        (company "Copyright (C) 2021 Tom Li (niconiconi)")
        (rev v0.01)
        (date 2021-06-29)
        (source usb-c.sch)
        (comment (number 1) (value https://creativecommons.org/publicdomain/zero/1.0/))
        (comment (number 2) (value "the designer has waived all copyright and related or neighboring rights."))
        (comment (number 3) (value "To the extent possible under law,"))
        (comment (number 4) (value "License: CC 0, “No Rights Reserved”"))))
    (sheet (number 3) (name /eeprom/) (tstamps /60B512DF/)
      (title_block
        (title "EEPROM and SPI Schematic - VL670 Development Board")
        (company "Copyright (C) 2021 Tom Li (niconiconi)")
        (rev v0.01)
        (date 2021-06-29)
        (source eeprom.sch)
        (comment (number 1) (value https://creativecommons.org/publicdomain/zero/1.0/))
        (comment (number 2) (value "the designer has waived all copyright and related or neighboring rights."))
        (comment (number 3) (value "To the extent possible under law,"))
        (comment (number 4) (value "License: CC 0, “No Rights Reserved”"))))
    (sheet (number 4) (name /layout/) (tstamps /60C6101E/)
      (title_block
        (title "PCB-specific Schematic - VL670 Development Board")
        (company "Copyright (C) 2021 Tom Li (niconiconi)")
        (rev v0.01)
        (date 2021-06-29)
        (source layout.sch)
        (comment (number 1) (value https://creativecommons.org/publicdomain/zero/1.0/))
        (comment (number 2) (value "the designer has waived all copyright and related or neighboring rights."))
        (comment (number 3) (value "To the extent possible under law,"))
        (comment (number 4) (value "License: CC 0, “No Rights Reserved”")))))
  (components
    (comp (ref R4)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FCCDE94))
    (comp (ref R6)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FD161E5))
    (comp (ref Y1)
      (value 25MHz)
      (footprint Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm)
      (datasheet ~)
      (fields
        (field (name Parameter) Cl=10pF))
      (libsource (lib Device) (part Crystal_GND24) (description "Four pin crystal, GND on pins 2 and 4"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F845F29))
    (comp (ref R5)
      (value 11.3k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Tolerance) 1%))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FE3B6E7))
    (comp (ref C13)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FCD98BF))
    (comp (ref J4)
      (value "USB3_A Receptacle")
      (footprint vl670:USB3_A_Receptacle_XKB_U231-091N-4BLRA00-S-1)
      (datasheet ~)
      (libsource (lib Connector) (part USB3_A) (description "USB 3.0 A connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604983E0))
    (comp (ref R7)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60761FDB))
    (comp (ref R8)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 607627E2))
    (comp (ref U4)
      (value TPS2061C-PXLI)
      (footprint Package_TO_SOT_SMD:SOT-23-5_HandSoldering)
      (datasheet https://www.ti.com/lit/gpn/tps2061c)
      (libsource (lib vl670) (part TPS2061C) (description "1.0A, 4.5-5.5V USB power switch, active-low enable, output discharge"))
      (sheetpath (names /) (tstamps /))
      (tstamp 605C86BA))
    (comp (ref R9)
      (value 470R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B5EC77))
    (comp (ref R3)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6026D222))
    (comp (ref C31)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602DF1BC))
    (comp (ref C32)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 602DF1D2))
    (comp (ref C33)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603DC68D))
    (comp (ref C34)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 603EC4B0))
    (comp (ref C41)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60400542))
    (comp (ref C42)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60400776))
    (comp (ref C43)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60400792))
    (comp (ref C44)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604007A2))
    (comp (ref C35)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604353DE))
    (comp (ref R2)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Install) NC))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6027F301))
    (comp (ref R1)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Install) NC))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6027A505))
    (comp (ref J2)
      (value USB_C_Receptacle)
      (footprint vl670:USB_C_Receptacle_XKB_U262-241N-4BV60)
      (datasheet https://www.usb.org/sites/default/files/documents/usb_type-c.zip)
      (libsource (lib Connector) (part USB_C_Receptacle) (description "USB Full-Featured Type-C Receptacle connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6001F703))
    (comp (ref D13)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF63F7))
    (comp (ref D15)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF6401))
    (comp (ref D16)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF640B))
    (comp (ref D17)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF641F))
    (comp (ref D14)
      (value ESD5B5.0ST1G-N)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF6415))
    (comp (ref JP2)
      (value SolderJumper_2_Bridged)
      (footprint Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Bridged) (description "Solder Jumper, 2-pole, closed/bridged"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61CB65FE))
    (comp (ref J5)
      (value Conn_01x02_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61A1F5FF))
    (comp (ref D18)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60EF6034))
    (comp (ref R15)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 608A3AA8))
    (comp (ref D3)
      (value ESD7104)
      (footprint vl670:OnSemi_UDFN-10_1.0x2.5mm_P0.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (libsource (lib vl670) (part ESD7104) (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10"))
      (sheetpath (names /) (tstamps /))
      (tstamp 604983EA))
    (comp (ref D2)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61B69FA3))
    (comp (ref U2)
      (value VL670)
      (footprint Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.3x4.3mm)
      (libsource (lib vl670) (part VL670) (description "USB 3 Super Speed to USB 2 High Speed Transaction Translator, VIA Labs, QFN-48"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FC75CE3))
    (comp (ref R19)
      (value 0R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6092DAD1))
    (comp (ref L1)
      (value 4.7uH)
      (footprint Inductor_SMD:L_1008_2520Metric_Pad1.43x2.20mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Brand) "L1: Sunlord")
        (field (name "Part Number") SPH252012H4R7MT))
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5FC96A7A))
    (comp (ref C61)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6054C690))
    (comp (ref C62)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6054C939))
    (comp (ref C11)
      (value 18pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Grade) NP0))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F845F1B))
    (comp (ref C10)
      (value 18pF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Grade) NP0))
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E741279))
    (comp (ref C8)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609AE51A))
    (comp (ref C7)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609AE13A))
    (comp (ref R20)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61D6C1E1))
    (comp (ref R21)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60D3D349))
    (comp (ref D6)
      (value ESD7104)
      (footprint vl670:OnSemi_UDFN-10_1.0x2.5mm_P0.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (libsource (lib vl670) (part ESD7104) (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6046BFCB))
    (comp (ref FB1)
      (value Ferrite_Bead_Small)
      (footprint Inductor_SMD:L_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6122E4EF))
    (comp (ref C20)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 608C5884))
    (comp (ref C52)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6069AFD4))
    (comp (ref C51)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6069AD6A))
    (comp (ref R23)
      (value 0R5)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 617165BA))
    (comp (ref C19)
      (value 10uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 608992C0))
    (comp (ref R22)
      (value 0R5)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 617B98B5))
    (comp (ref J3)
      (value Conn_01x08_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x08_Male) (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 613F2C9C))
    (comp (ref R13)
      (value 470R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6155423C))
    (comp (ref D12)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609A27AC))
    (comp (ref D11)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609A27A2))
    (comp (ref D10)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 609A2548))
    (comp (ref D9)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6098C822))
    (comp (ref D8)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60976B35))
    (comp (ref D7)
      (value ESD5B5.0ST1G-N)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60915659))
    (comp (ref D19)
      (value ESD7951S)
      (footprint Diode_SMD:D_SOD-523)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61757663))
    (comp (ref D20)
      (value LED)
      (footprint LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part LED) (description "Light emitting diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6141C9C6))
    (comp (ref R24)
      (value 470R)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6141EC3B))
    (comp (ref J1)
      (value Conn_01x07_Male)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x07_Male) (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 60C3937B))
    (comp (ref D1)
      (value ESD7104)
      (footprint vl670:OnSemi_UDFN-10_1.0x2.5mm_P0.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (libsource (lib vl670) (part ESD7104) (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 604F2862))
    (comp (ref D4)
      (value ESD7104)
      (footprint vl670:OnSemi_UDFN-10_1.0x2.5mm_P0.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (libsource (lib vl670) (part ESD7104) (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60535F6E))
    (comp (ref R12)
      (value 1.8M)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Tolerance) 1%))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 5FD0592B))
    (comp (ref R14)
      (value 200k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 5FD868A6))
    (comp (ref D5)
      (value ESD7104)
      (footprint vl670:OnSemi_UDFN-10_1.0x2.5mm_P0.5mm)
      (datasheet https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (libsource (lib vl670) (part ESD7104) (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 5FFD97ED))
    (comp (ref C25)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 5FE72F82))
    (comp (ref C12)
      (value 1uF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 5FE7CBDA))
    (comp (ref C5)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60F44413))
    (comp (ref C6)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60F44419))
    (comp (ref R16)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60B29DEF))
    (comp (ref R17)
      (value 100K)
      (footprint Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60B2F7A0))
    (comp (ref U1)
      (value HD3SS3220)
      (footprint vl670:Texas_VQFN-RNH-30)
      (libsource (lib vl670) (part HD3SS3220) (description "USB Type-C DRP Port Controller with SuperSpeed 2:1 MUX, Texas Instruments, VQFN-30"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60228179))
    (comp (ref C4)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60EF5296))
    (comp (ref R18)
      (value 1.8M)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (fields
        (field (name Tolerance) 1%))
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60BFA35D))
    (comp (ref C3)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60EF5290))
    (comp (ref C2)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60EF52A2))
    (comp (ref C1)
      (value 220nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names "/USB AC CAP/ESD/MUX/") (tstamps /60085564/))
      (tstamp 60EF529C))
    (comp (ref U6)
      (value GD25D05)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet http://www.ti.com/lit/ds/symlink/cd4016b.pdf)
      (libsource (lib vl670) (part 25LCxxx) (description "SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61456C68))
    (comp (ref R10)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61456C7C))
    (comp (ref C22)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61456C9A))
    (comp (ref R11)
      (value 10k)
      (footprint Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_US) (description "Resistor, US symbol"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 607E550A))
    (comp (ref JP1)
      (value SolderJumper_2_Open)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 6086203D))
    (comp (ref C26)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 607CC437))
    (comp (ref U3)
      (value 74LVC2G66)
      (footprint Package_SO:VSSOP-8_2.4x2.1mm_P0.5mm)
      (datasheet https://assets.nexperia.com/documents/data-sheet/74LVC2G66.pdf)
      (libsource (lib vl670) (part 74LVC2G66) (description "Dual Analog Switches"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61B0808D))
    (comp (ref U5)
      (value 74LVC2G66)
      (footprint Package_SO:VSSOP-8_2.4x2.1mm_P0.5mm)
      (datasheet https://assets.nexperia.com/documents/data-sheet/74LVC2G66.pdf)
      (libsource (lib vl670) (part 74LVC2G66) (description "Dual Analog Switches"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61B0C3AB))
    (comp (ref C9)
      (value 470nF)
      (footprint Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /eeprom/) (tstamps /60B512DF/))
      (tstamp 61B10967))
    (comp (ref C73)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CBBE89))
    (comp (ref C74)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CBD769))
    (comp (ref C75)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CD8243))
    (comp (ref C76)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CD82EB))
    (comp (ref C77)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CD82FA))
    (comp (ref C78)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CD8311))
    (comp (ref C79)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609B2CD4))
    (comp (ref C80)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609B2DF2))
    (comp (ref C81)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609B2E01))
    (comp (ref C82)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609B2E17))
    (comp (ref C72)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CBBE7E))
    (comp (ref C71)
      (value 470nF)
      (footprint Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C) (description "Unpolarized capacitor"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 60CBBE70))
    (comp (ref FID8)
      (value Fiducial)
      (footprint vl670:StencilFiducial_0.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609F6765))
    (comp (ref FID6)
      (value Fiducial)
      (footprint vl670:StencilFiducial_0.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609F675B))
    (comp (ref FID4)
      (value Fiducial)
      (footprint vl670:StencilFiducial_0.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609F6751))
    (comp (ref FID2)
      (value Fiducial)
      (footprint vl670:StencilFiducial_0.5mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609F668F))
    (comp (ref FID7)
      (value Fiducial)
      (footprint vl670:StencilFiducial_1mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609E8380))
    (comp (ref FID5)
      (value Fiducial)
      (footprint vl670:StencilFiducial_1mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609E81CA))
    (comp (ref FID3)
      (value Fiducial)
      (footprint vl670:StencilFiducial_1mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609E4349))
    (comp (ref FID1)
      (value Fiducial)
      (footprint vl670:StencilFiducial_1mm)
      (datasheet ~)
      (libsource (lib Mechanical) (part Fiducial) (description "Fiducial Marker"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 609E1399))
    (comp (ref TP1)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (fields
        (field (name Marking) 3V3))
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 613E415B))
    (comp (ref TP2)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 613E8124))
    (comp (ref TP3)
      (value TestPoint)
      (footprint TestPoint:TestPoint_Pad_D1.0mm)
      (datasheet ~)
      (fields
        (field (name Marking) 1V2))
      (libsource (lib Connector) (part TestPoint) (description "test point"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 613EE06A))
    (comp (ref H1)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_2.5mm_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 614F95F3))
    (comp (ref H2)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_2.5mm_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 614FB012))
    (comp (ref H3)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_2.5mm_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 614FDAB8))
    (comp (ref H4)
      (value MountingHole_Pad)
      (footprint MountingHole:MountingHole_2.5mm_Pad_Via)
      (datasheet ~)
      (libsource (lib Mechanical) (part MountingHole_Pad) (description "Mounting Hole with connection"))
      (sheetpath (names /layout/) (tstamps /60C6101E/))
      (tstamp 61500BBD)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x07_Male)
      (description "Generic connector, single row, 01x07, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x07_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))))
    (libpart (lib Connector) (part Conn_01x08_Male)
      (description "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector) (part TestPoint)
      (description "test point")
      (docs ~)
      (footprints
        (fp Pin*)
        (fp Test*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TestPoint))
      (pins
        (pin (num 1) (name 1) (type passive))))
    (libpart (lib Connector) (part USB3_A)
      (description "USB 3.0 A connector")
      (docs ~)
      (fields
        (field (name Reference) J)
        (field (name Value) USB3_A))
      (pins
        (pin (num 1) (name VBUS) (type power_in))
        (pin (num 2) (name D-) (type BiDi))
        (pin (num 3) (name D+) (type BiDi))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name SSRX-) (type output))
        (pin (num 6) (name SSRX+) (type output))
        (pin (num 7) (name DRAIN) (type passive))
        (pin (num 8) (name SSTX-) (type input))
        (pin (num 9) (name SSTX+) (type input))
        (pin (num 10) (name SHIELD) (type passive))))
    (libpart (lib Connector) (part USB_C_Receptacle)
      (description "USB Full-Featured Type-C Receptacle connector")
      (docs https://www.usb.org/sites/default/files/documents/usb_type-c.zip)
      (footprints
        (fp USB*C*Receptacle*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_C_Receptacle))
      (pins
        (pin (num A1) (name GND) (type passive))
        (pin (num A2) (name TX1+) (type BiDi))
        (pin (num A3) (name TX1-) (type BiDi))
        (pin (num A4) (name VBUS) (type passive))
        (pin (num A5) (name CC1) (type BiDi))
        (pin (num A6) (name D+) (type BiDi))
        (pin (num A7) (name D-) (type BiDi))
        (pin (num A8) (name SBU1) (type BiDi))
        (pin (num A9) (name VBUS) (type passive))
        (pin (num A10) (name RX2-) (type BiDi))
        (pin (num A11) (name RX2+) (type BiDi))
        (pin (num A12) (name GND) (type passive))
        (pin (num B1) (name GND) (type passive))
        (pin (num B2) (name TX2+) (type BiDi))
        (pin (num B3) (name TX2-) (type BiDi))
        (pin (num B4) (name VBUS) (type passive))
        (pin (num B5) (name CC2) (type BiDi))
        (pin (num B6) (name D+) (type BiDi))
        (pin (num B7) (name D-) (type BiDi))
        (pin (num B8) (name SBU2) (type BiDi))
        (pin (num B9) (name VBUS) (type passive))
        (pin (num B10) (name RX1-) (type BiDi))
        (pin (num B11) (name RX1+) (type BiDi))
        (pin (num B12) (name GND) (type passive))
        (pin (num S1) (name SHIELD) (type passive))))
    (libpart (lib Device) (part C)
      (description "Unpolarized capacitor")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_GND24)
      (description "Four pin crystal, GND on pins 2 and 4")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib Device) (part D_TVS)
      (description "Bidirectional transient-voltage-suppression diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_TVS))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part LED)
      (description "Light emitting diode")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part L_Small)
      (description "Inductor, small symbol")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_US)
      (description "Resistor, US symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_US))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Bridged)
      (description "Solder Jumper, 2-pole, closed/bridged")
      (docs ~)
      (footprints
        (fp SolderJumper*Bridged*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Bridged))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Jumper) (part SolderJumper_2_Open)
      (description "Solder Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib Mechanical) (part Fiducial)
      (description "Fiducial Marker")
      (docs ~)
      (footprints
        (fp Fiducial*))
      (fields
        (field (name Reference) FID)
        (field (name Value) Fiducial)))
    (libpart (lib Mechanical) (part MountingHole_Pad)
      (description "Mounting Hole with connection")
      (docs ~)
      (footprints
        (fp MountingHole*Pad*))
      (fields
        (field (name Reference) H)
        (field (name Value) MountingHole_Pad))
      (pins
        (pin (num 1) (name 1) (type input))))
    (libpart (lib vl670) (part 25LCxxx)
      (aliases
        (alias BR25Sxxx)
        (alias CAT250xxx)
        (alias AT25xxx))
      (description "SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf)
      (footprints
        (fp DIP*W7.62mm*)
        (fp SOIC*3.9x4.9mm*)
        (fp TSSOP*4.4x3mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) 25LCxxx))
      (pins
        (pin (num 1) (name ~CS) (type input))
        (pin (num 2) (name MISO) (type 3state))
        (pin (num 3) (name ~WP) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name MOSI) (type input))
        (pin (num 6) (name SCK) (type input))
        (pin (num 7) (name ~HOLD) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib vl670) (part 74LVC2G66)
      (description "Dual Analog Switches")
      (docs https://assets.nexperia.com/documents/data-sheet/74LVC2G66.pdf)
      (footprints
        (fp VSSOP?8*))
      (fields
        (field (name Reference) U)
        (field (name Value) 74LVC2G66))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type input))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type input))
        (pin (num 8) (name VCC) (type power_in))))
    (libpart (lib vl670) (part ESD7104)
      (description "Low Capacitance ESD Protection Diodefor High Speed Data Line, 2 Channels, UDFN-10/WDFNW-10")
      (docs https://www.onsemi.com/pub/Collateral/ESD7104-D.PDF)
      (footprints
        (fp Diodes_UDFN-10_1.0x2.5mm_P0.5mm))
      (fields
        (field (name Reference) D)
        (field (name Value) ESD7104)
        (field (name Footprint) Package_DFN_QFN:Diodes_UDFN-10_1.0x2.5mm_P0.5mm))
      (pins
        (pin (num 1) (name TVS1) (type passive))
        (pin (num 2) (name TVS2) (type passive))
        (pin (num 3) (name COM) (type passive))
        (pin (num 4) (name TVS3) (type passive))
        (pin (num 5) (name TVS4) (type passive))
        (pin (num 6) (name NC4) (type passive))
        (pin (num 7) (name NC3) (type passive))
        (pin (num 8) (name GND) (type passive))
        (pin (num 9) (name NC2) (type passive))
        (pin (num 10) (name NC1) (type passive))))
    (libpart (lib vl670) (part HD3SS3220)
      (description "USB Type-C DRP Port Controller with SuperSpeed 2:1 MUX, Texas Instruments, VQFN-30")
      (footprints
        (fp QFN*1EP*6x6mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) HD3SS3220))
      (pins
        (pin (num 1) (name CC2) (type BiDi))
        (pin (num 2) (name CC1) (type BiDi))
        (pin (num 3) (name CURRENT_MODE) (type input))
        (pin (num 4) (name PORT) (type input))
        (pin (num 5) (name VBUS_DET) (type input))
        (pin (num 6) (name TX-) (type passive))
        (pin (num 7) (name TX+) (type passive))
        (pin (num 8) (name VCC33) (type power_in))
        (pin (num 9) (name RX-) (type passive))
        (pin (num 10) (name RX+) (type passive))
        (pin (num 11) (name DIR) (type output))
        (pin (num 12) (name ~EN_MUX) (type input))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name RX1-) (type passive))
        (pin (num 15) (name RX1+) (type passive))
        (pin (num 16) (name TX1-) (type passive))
        (pin (num 17) (name TX1+) (type passive))
        (pin (num 18) (name RX2-) (type passive))
        (pin (num 19) (name RX2+) (type passive))
        (pin (num 20) (name TX2-) (type passive))
        (pin (num 21) (name TX2+) (type passive))
        (pin (num 22) (name ADDR) (type input))
        (pin (num 23) (name ~INT_N~/OUT3) (type output))
        (pin (num 24) (name ~VCONN_FAULT) (type output))
        (pin (num 25) (name SDA/OUT1) (type BiDi))
        (pin (num 26) (name SCL/OUT2) (type BiDi))
        (pin (num 27) (name ID) (type output))
        (pin (num 28) (name GND) (type power_in))
        (pin (num 29) (name ~EN_CC) (type input))
        (pin (num 30) (name VDD5) (type power_in))
        (pin (num 31) (name GND) (type power_in))))
    (libpart (lib vl670) (part TPS2061C)
      (description "1.0A, 4.5-5.5V USB power switch, active-low enable, output discharge")
      (docs https://www.ti.com/lit/gpn/tps2061c)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) TPS2061C)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name OUT) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name ~FAULT) (type openCol))
        (pin (num 4) (name ~EN) (type input))
        (pin (num 5) (name IN) (type power_in))))
    (libpart (lib vl670) (part VL670)
      (description "USB 3 Super Speed to USB 2 High Speed Transaction Translator, VIA Labs, QFN-48")
      (footprints
        (fp QFN*1EP*6x6mm*P0.4mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) VL670))
      (pins
        (pin (num 1) (name DCGND) (type power_in))
        (pin (num 2) (name LX) (type power_out))
        (pin (num 3) (name DCVDD5) (type power_in))
        (pin (num 4) (name GPIO3_0/STATUS) (type BiDi))
        (pin (num 5) (name VCC33) (type power_in))
        (pin (num 6) (name GPIO2_1/UART_TX) (type BiDi))
        (pin (num 7) (name GPIO2_0/UART_RX) (type BiDi))
        (pin (num 8) (name TESTEN) (type input))
        (pin (num 9) (name LDOVDD33O) (type power_out))
        (pin (num 10) (name LDOVDD5) (type power_in))
        (pin (num 11) (name REXT) (type input))
        (pin (num 12) (name MVDD15) (type power_in))
        (pin (num 13) (name UP_USB3TX-) (type output))
        (pin (num 14) (name UP_USB3TX+) (type output))
        (pin (num 15) (name U3TXAVDD15) (type power_in))
        (pin (num 16) (name DN_USB3RX-) (type input))
        (pin (num 17) (name DN_USB3RX+) (type input))
        (pin (num 18) (name UP_USB3RX-) (type input))
        (pin (num 19) (name UP_USB3RX+) (type input))
        (pin (num 20) (name U3RXAVDD15) (type power_in))
        (pin (num 21) (name DN_USB3TX-) (type output))
        (pin (num 22) (name DN_USB3TX+) (type output))
        (pin (num 23) (name DN_D+) (type BiDi))
        (pin (num 24) (name DN_D-) (type BiDi))
        (pin (num 25) (name UP_D-) (type BiDi))
        (pin (num 26) (name UP_D+) (type BiDi))
        (pin (num 27) (name VCCU33) (type power_in))
        (pin (num 28) (name XO) (type output))
        (pin (num 29) (name XI) (type input))
        (pin (num 30) (name VDD12) (type power_in))
        (pin (num 31) (name STRP2) (type input))
        (pin (num 32) (name STRP1) (type input))
        (pin (num 33) (name STRP0) (type input))
        (pin (num 34) (name ~RESET~) (type input))
        (pin (num 35) (name VCC33) (type power_in))
        (pin (num 36) (name GPIO1_1/GPIO_TP2) (type BiDi))
        (pin (num 37) (name GPIO1_3/DN_PWREN) (type BiDi))
        (pin (num 38) (name GPIO1_2/GPIO_TP3) (type BiDi))
        (pin (num 39) (name GPIO1_0/GPIO_TP1) (type BiDi))
        (pin (num 40) (name SPI_SCLK) (type output))
        (pin (num 41) (name ~SPI_SS) (type output))
        (pin (num 42) (name SPI_MOSI) (type output))
        (pin (num 43) (name SPI_MISO) (type input))
        (pin (num 44) (name VCC33) (type power_in))
        (pin (num 45) (name GPIO3_1/GPIO_TP4) (type BiDi))
        (pin (num 46) (name LDOVDD12O) (type power_out))
        (pin (num 47) (name LDOVDD15) (type power_in))
        (pin (num 48) (name DCVDD15FB) (type input))
        (pin (num 49) (name GND) (type power_in)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library/Connector.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Jumper)
      (uri /usr/share/kicad/library/Jumper.lib))
    (library (logical Mechanical)
      (uri /usr/share/kicad/library/Mechanical.lib))
    (library (logical vl670)
      (uri /home/user/QubesIncoming/crypto/pcb/hisolator/vl670/vl670/vl670.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref R24) (pin 2))
      (node (ref D17) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref J4) (pin 4))
      (node (ref J4) (pin 7))
      (node (ref R7) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref D19) (pin 2))
      (node (ref J1) (pin 7))
      (node (ref D14) (pin 2))
      (node (ref D9) (pin 2))
      (node (ref D10) (pin 2))
      (node (ref D11) (pin 2))
      (node (ref D12) (pin 2))
      (node (ref J5) (pin 2))
      (node (ref J2) (pin A12))
      (node (ref J2) (pin A1))
      (node (ref J2) (pin B1))
      (node (ref J2) (pin B12))
      (node (ref D16) (pin 2))
      (node (ref D3) (pin 8))
      (node (ref R15) (pin 2))
      (node (ref D3) (pin 3))
      (node (ref J4) (pin 10))
      (node (ref D18) (pin 2))
      (node (ref J3) (pin 8))
      (node (ref D7) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref C44) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref C42) (pin 2))
      (node (ref C43) (pin 2))
      (node (ref C35) (pin 2))
      (node (ref C32) (pin 2))
      (node (ref C31) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref R23) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref R22) (pin 2))
      (node (ref C51) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref D6) (pin 8))
      (node (ref D6) (pin 3))
      (node (ref Y1) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref C52) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref Y1) (pin 4))
      (node (ref C71) (pin 2))
      (node (ref C72) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref H4) (pin 1))
      (node (ref H3) (pin 1))
      (node (ref H2) (pin 1))
      (node (ref H1) (pin 1))
      (node (ref C22) (pin 2))
      (node (ref U6) (pin 4))
      (node (ref C10) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C62) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref C61) (pin 2))
      (node (ref C81) (pin 2))
      (node (ref C80) (pin 2))
      (node (ref C82) (pin 2))
      (node (ref C79) (pin 2))
      (node (ref C78) (pin 2))
      (node (ref C77) (pin 2))
      (node (ref C76) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref C75) (pin 2))
      (node (ref C74) (pin 2))
      (node (ref U2) (pin 49))
      (node (ref C73) (pin 2))
      (node (ref D1) (pin 3))
      (node (ref D1) (pin 8))
      (node (ref D4) (pin 3))
      (node (ref C25) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref D13) (pin 2))
      (node (ref D15) (pin 2))
      (node (ref J2) (pin S1))
      (node (ref U1) (pin 13))
      (node (ref U1) (pin 12))
      (node (ref R17) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 28))
      (node (ref U1) (pin 29))
      (node (ref U1) (pin 31))
      (node (ref D4) (pin 8))
      (node (ref U3) (pin 4))
      (node (ref U5) (pin 4))
      (node (ref C9) (pin 2))
      (node (ref C12) (pin 2))
      (node (ref D5) (pin 8))
      (node (ref D5) (pin 3))
      (node (ref JP1) (pin 2))
      (node (ref C26) (pin 2)))
    (net (code 2) (name "Net-(L1-Pad2)")
      (node (ref L1) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 3) (name "Net-(R19-Pad1)")
      (node (ref U2) (pin 8))
      (node (ref R19) (pin 1)))
    (net (code 4) (name /SSRX_DEMUX+)
      (node (ref U2) (pin 19))
      (node (ref U1) (pin 10)))
    (net (code 5) (name /SSRX_DEMUX-)
      (node (ref U2) (pin 18))
      (node (ref U1) (pin 9)))
    (net (code 6) (name "Net-(D11-Pad1)")
      (node (ref D11) (pin 1))
      (node (ref J3) (pin 6))
      (node (ref U2) (pin 6)))
    (net (code 7) (name "Net-(D10-Pad1)")
      (node (ref J3) (pin 5))
      (node (ref D10) (pin 1))
      (node (ref U2) (pin 7)))
    (net (code 8) (name +1V2)
      (node (ref TP3) (pin 1))
      (node (ref C61) (pin 1))
      (node (ref C62) (pin 1))
      (node (ref U2) (pin 30))
      (node (ref U2) (pin 46)))
    (net (code 9) (name ~EXT_RESET)
      (node (ref U2) (pin 34))
      (node (ref C13) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U3) (pin 3))
      (node (ref R3) (pin 2))
      (node (ref U3) (pin 7))
      (node (ref J1) (pin 6))
      (node (ref U5) (pin 7))
      (node (ref U5) (pin 3))
      (node (ref D17) (pin 1)))
    (net (code 10) (name "Net-(R15-Pad1)")
      (node (ref U2) (pin 37))
      (node (ref R15) (pin 1))
      (node (ref U4) (pin 4)))
    (net (code 11) (name +5V)
      (node (ref J5) (pin 1))
      (node (ref D18) (pin 1))
      (node (ref C51) (pin 1))
      (node (ref U2) (pin 10))
      (node (ref R18) (pin 2))
      (node (ref C52) (pin 1))
      (node (ref JP2) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref C19) (pin 1))
      (node (ref U2) (pin 3))
      (node (ref U4) (pin 5))
      (node (ref U1) (pin 30)))
    (net (code 12) (name "Net-(D2-Pad2)")
      (node (ref R13) (pin 1))
      (node (ref R9) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 13) (name "/USB AC CAP/ESD/MUX/TX1-")
      (node (ref C1) (pin 2))
      (node (ref J2) (pin A3))
      (node (ref D1) (pin 5))
      (node (ref D1) (pin 6)))
    (net (code 14) (name "/USB AC CAP/ESD/MUX/TX1+")
      (node (ref J2) (pin A2))
      (node (ref D1) (pin 7))
      (node (ref D1) (pin 4))
      (node (ref C2) (pin 2)))
    (net (code 15) (name "/USB AC CAP/ESD/MUX/TX2-")
      (node (ref D4) (pin 7))
      (node (ref D4) (pin 4))
      (node (ref J2) (pin B3))
      (node (ref C4) (pin 2)))
    (net (code 16) (name "/USB AC CAP/ESD/MUX/TX2+")
      (node (ref C3) (pin 2))
      (node (ref D4) (pin 5))
      (node (ref J2) (pin B2))
      (node (ref D4) (pin 6)))
    (net (code 17) (name "/USB AC CAP/ESD/MUX/RX2+")
      (node (ref D4) (pin 9))
      (node (ref D4) (pin 2))
      (node (ref U1) (pin 19))
      (node (ref J2) (pin A11)))
    (net (code 18) (name "/USB AC CAP/ESD/MUX/RX2-")
      (node (ref D4) (pin 10))
      (node (ref D4) (pin 1))
      (node (ref J2) (pin A10))
      (node (ref U1) (pin 18)))
    (net (code 19) (name /D_DEMUX+)
      (node (ref U2) (pin 26))
      (node (ref R2) (pin 1)))
    (net (code 20) (name "Net-(C11-Pad1)")
      (node (ref U2) (pin 28))
      (node (ref C11) (pin 1))
      (node (ref Y1) (pin 1)))
    (net (code 21) (name "Net-(C10-Pad1)")
      (node (ref U2) (pin 29))
      (node (ref Y1) (pin 3))
      (node (ref C10) (pin 1)))
    (net (code 22) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 33)))
    (net (code 23) (name "Net-(D8-Pad1)")
      (node (ref R21) (pin 1))
      (node (ref D8) (pin 1))
      (node (ref U2) (pin 39))
      (node (ref J3) (pin 3)))
    (net (code 24) (name /eeprom/SCK)
      (node (ref U3) (pin 5))
      (node (ref U2) (pin 40)))
    (net (code 25) (name /eeprom/~CS)
      (node (ref U3) (pin 1))
      (node (ref U2) (pin 41)))
    (net (code 26) (name /eeprom/MOSI)
      (node (ref U2) (pin 42))
      (node (ref U5) (pin 5)))
    (net (code 27) (name /eeprom/MISO)
      (node (ref U5) (pin 1))
      (node (ref U2) (pin 43)))
    (net (code 28) (name "Net-(D12-Pad1)")
      (node (ref D12) (pin 1))
      (node (ref U2) (pin 45))
      (node (ref J3) (pin 7)))
    (net (code 29) (name "Net-(D19-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref D19) (pin 1))
      (node (ref U2) (pin 4))
      (node (ref R13) (pin 2)))
    (net (code 30) (name "Net-(D7-Pad1)")
      (node (ref R9) (pin 2))
      (node (ref U2) (pin 36))
      (node (ref D7) (pin 1))
      (node (ref J3) (pin 2)))
    (net (code 31) (name "Net-(D20-Pad1)")
      (node (ref D20) (pin 1))
      (node (ref R24) (pin 1)))
    (net (code 32) (name /eeprom/~ISP_CS)
      (node (ref D13) (pin 1))
      (node (ref U6) (pin 1))
      (node (ref U3) (pin 2))
      (node (ref J1) (pin 3)))
    (net (code 33) (name /eeprom/ISP_MOSI)
      (node (ref D15) (pin 1))
      (node (ref U5) (pin 6))
      (node (ref U6) (pin 5))
      (node (ref J1) (pin 5)))
    (net (code 34) (name "Net-(D9-Pad1)")
      (node (ref R20) (pin 1))
      (node (ref J3) (pin 4))
      (node (ref D9) (pin 1))
      (node (ref U2) (pin 38)))
    (net (code 35) (name +5V_SW)
      (node (ref D3) (pin 2))
      (node (ref D20) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref D3) (pin 9))
      (node (ref D3) (pin 10))
      (node (ref C20) (pin 1))
      (node (ref U4) (pin 1))
      (node (ref J4) (pin 1)))
    (net (code 36) (name "Net-(C20-Pad2)")
      (node (ref R23) (pin 1))
      (node (ref C20) (pin 2)))
    (net (code 37) (name +5VP)
      (node (ref J2) (pin A9))
      (node (ref FB1) (pin 2))
      (node (ref J2) (pin A4))
      (node (ref J2) (pin B9))
      (node (ref J2) (pin B4)))
    (net (code 38) (name "Net-(U4-Pad3)")
      (node (ref U4) (pin 3)))
    (net (code 39) (name /DN_TX_AC-)
      (node (ref D6) (pin 10))
      (node (ref C7) (pin 1))
      (node (ref D6) (pin 1))
      (node (ref J4) (pin 9)))
    (net (code 40) (name /DN_TX_AC+)
      (node (ref D6) (pin 9))
      (node (ref C8) (pin 1))
      (node (ref D6) (pin 2))
      (node (ref J4) (pin 8)))
    (net (code 41) (name "Net-(FB1-Pad1)")
      (node (ref JP2) (pin 1))
      (node (ref FB1) (pin 1)))
    (net (code 42) (name "Net-(C19-Pad2)")
      (node (ref R22) (pin 1))
      (node (ref C19) (pin 2)))
    (net (code 43) (name /D_DEMUX-)
      (node (ref R1) (pin 1))
      (node (ref U2) (pin 25)))
    (net (code 44) (name +1V5)
      (node (ref C42) (pin 1))
      (node (ref L1) (pin 1))
      (node (ref U2) (pin 48))
      (node (ref U2) (pin 20))
      (node (ref U2) (pin 47))
      (node (ref U2) (pin 12))
      (node (ref TP2) (pin 1))
      (node (ref C43) (pin 1))
      (node (ref U2) (pin 15))
      (node (ref C44) (pin 1))
      (node (ref C41) (pin 1)))
    (net (code 45) (name +3V3)
      (node (ref U3) (pin 8))
      (node (ref U2) (pin 27))
      (node (ref C31) (pin 1))
      (node (ref C25) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C81) (pin 1))
      (node (ref C74) (pin 1))
      (node (ref C80) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref C33) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref U2) (pin 44))
      (node (ref C79) (pin 1))
      (node (ref U5) (pin 8))
      (node (ref C26) (pin 1))
      (node (ref C77) (pin 1))
      (node (ref C72) (pin 1))
      (node (ref C71) (pin 1))
      (node (ref C35) (pin 1))
      (node (ref TP1) (pin 1))
      (node (ref U6) (pin 8))
      (node (ref C78) (pin 1))
      (node (ref C82) (pin 1))
      (node (ref C73) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref C76) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref U2) (pin 5))
      (node (ref R10) (pin 1))
      (node (ref U2) (pin 35))
      (node (ref C9) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref C75) (pin 1))
      (node (ref C22) (pin 1)))
    (net (code 46) (name "Net-(R5-Pad1)")
      (node (ref U2) (pin 11))
      (node (ref R5) (pin 1)))
    (net (code 47) (name "Net-(R7-Pad1)")
      (node (ref R7) (pin 1))
      (node (ref U2) (pin 32)))
    (net (code 48) (name "Net-(R8-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref U2) (pin 31)))
    (net (code 49) (name /eeprom/ISP_SCK)
      (node (ref U3) (pin 6))
      (node (ref J1) (pin 2))
      (node (ref D14) (pin 1))
      (node (ref U6) (pin 6)))
    (net (code 50) (name /eeprom/ISP_MISO)
      (node (ref U5) (pin 2))
      (node (ref U6) (pin 2))
      (node (ref J1) (pin 4))
      (node (ref D16) (pin 1)))
    (net (code 51) (name "/USB AC CAP/ESD/MUX/RX1-")
      (node (ref J2) (pin B10))
      (node (ref D1) (pin 9))
      (node (ref U1) (pin 15))
      (node (ref D1) (pin 2)))
    (net (code 52) (name "/USB AC CAP/ESD/MUX/CC2")
      (node (ref D5) (pin 2))
      (node (ref J2) (pin B5))
      (node (ref D5) (pin 9))
      (node (ref U1) (pin 1)))
    (net (code 53) (name "/USB AC CAP/ESD/MUX/CC1")
      (node (ref J2) (pin A5))
      (node (ref D5) (pin 1))
      (node (ref D5) (pin 10))
      (node (ref U1) (pin 2)))
    (net (code 54) (name "/USB AC CAP/ESD/MUX/RX1+")
      (node (ref J2) (pin B11))
      (node (ref U1) (pin 14))
      (node (ref D1) (pin 10))
      (node (ref D1) (pin 1)))
    (net (code 55) (name "Net-(J2-PadA8)")
      (node (ref J2) (pin A8)))
    (net (code 56) (name "Net-(J2-PadB8)")
      (node (ref J2) (pin B8)))
    (net (code 57) (name "/USB AC CAP/ESD/MUX/D-")
      (node (ref J2) (pin B7))
      (node (ref R1) (pin 2))
      (node (ref J2) (pin A7))
      (node (ref D5) (pin 5))
      (node (ref D5) (pin 6)))
    (net (code 58) (name "/USB AC CAP/ESD/MUX/D+")
      (node (ref J2) (pin B6))
      (node (ref D5) (pin 4))
      (node (ref J2) (pin A6))
      (node (ref R2) (pin 2))
      (node (ref D5) (pin 7)))
    (net (code 59) (name /DN_SSTX+)
      (node (ref C8) (pin 2))
      (node (ref U2) (pin 22)))
    (net (code 60) (name /DN_SSTX-)
      (node (ref U2) (pin 21))
      (node (ref C7) (pin 2)))
    (net (code 61) (name /DN_SSRX+)
      (node (ref J4) (pin 6))
      (node (ref D6) (pin 6))
      (node (ref D6) (pin 5))
      (node (ref U2) (pin 17)))
    (net (code 62) (name /DN_SSRX-)
      (node (ref J4) (pin 5))
      (node (ref D6) (pin 4))
      (node (ref D6) (pin 7))
      (node (ref U2) (pin 16)))
    (net (code 63) (name /DN_D+)
      (node (ref U2) (pin 23))
      (node (ref D3) (pin 6))
      (node (ref D3) (pin 5))
      (node (ref J4) (pin 3)))
    (net (code 64) (name /DN_D-)
      (node (ref U2) (pin 24))
      (node (ref D3) (pin 4))
      (node (ref D3) (pin 7))
      (node (ref J4) (pin 2)))
    (net (code 65) (name /SSTX_DEMUX+)
      (node (ref U2) (pin 13))
      (node (ref C6) (pin 1)))
    (net (code 66) (name /SSTX_DEMUX-)
      (node (ref U2) (pin 14))
      (node (ref C5) (pin 1)))
    (net (code 67) (name "Net-(R14-Pad1)")
      (node (ref U1) (pin 11))
      (node (ref R14) (pin 1)))
    (net (code 68) (name "/USB AC CAP/ESD/MUX/TX_MUX_DC-")
      (node (ref R16) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref U1) (pin 6)))
    (net (code 69) (name "Net-(U1-Pad27)")
      (node (ref U1) (pin 27)))
    (net (code 70) (name "Net-(R12-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref R12) (pin 1))
      (node (ref R18) (pin 1)))
    (net (code 71) (name "/USB AC CAP/ESD/MUX/TX_MUX_DC+")
      (node (ref U1) (pin 7))
      (node (ref R17) (pin 1))
      (node (ref C6) (pin 2)))
    (net (code 72) (name "Net-(U1-Pad22)")
      (node (ref U1) (pin 22)))
    (net (code 73) (name "Net-(U1-Pad23)")
      (node (ref U1) (pin 23)))
    (net (code 74) (name "Net-(U1-Pad24)")
      (node (ref U1) (pin 24)))
    (net (code 75) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 76) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 77) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 78) (name "/USB AC CAP/ESD/MUX/TX1_AC+")
      (node (ref U1) (pin 16))
      (node (ref C2) (pin 1)))
    (net (code 79) (name "/USB AC CAP/ESD/MUX/TX2_AC-")
      (node (ref U1) (pin 20))
      (node (ref C4) (pin 1)))
    (net (code 80) (name "/USB AC CAP/ESD/MUX/TX2_AC+")
      (node (ref C3) (pin 1))
      (node (ref U1) (pin 21)))
    (net (code 81) (name "/USB AC CAP/ESD/MUX/TX1_AC-")
      (node (ref U1) (pin 17))
      (node (ref C1) (pin 1)))
    (net (code 82) (name "Net-(JP1-Pad1)")
      (node (ref R11) (pin 2))
      (node (ref JP1) (pin 1))
      (node (ref U6) (pin 3)))
    (net (code 83) (name "Net-(R10-Pad2)")
      (node (ref U6) (pin 7))
      (node (ref R10) (pin 2)))))